|  |  |
| --- | --- |
| **Landowner Information** | **Responsible Party Information**  **(Erosion & Sediment Control)** |
| **Name (List both the company name and individual name if applicable)** | **Name (List both the company name and individual name if applicable)** |
| **Address** | **Address** |
| **Phone** | **Phone** |
| **Fax** | **Fax** |
| **Email** | **Email** |
| **Location of Proposed New Single Family Home Construction (Address, PIN, Map Number)** | |

**Agreement**

In lieu of submission of an Erosion and Sediment Control Plan for the construction of this new single-family residence, I (the property owner) agree to comply with any requirements determined necessary by the City of Danville Combined Administrator or his designee. Such requirements shall be based on the standards of the City of Danville’s Erosion and Sediment Control Ordinance, and shall represent the minimum practices necessary to provide adequate control of erosion and sedimentation on or resulting from this project. I further understand that failure to comply with such requirements within **three calendar days** following notification from the Combined Administrator or his designee may result in citation for violation of the City of Danville’s Erosion and Sediment Control Ordinance.

At a minimum, the following erosion and sediment controls will be utilized:

* Construction entrances at all points of egress from the project.
* Silt fence installed at the lower side of all disturbed areas.
* Temporary seeding on disturbed areas that are left dormant for more than 30 days.
* Permanent seeding on all disturbed areas within 7 days after final grade is achieved.

This Agreement does not relieve the owner of any requirements to submit other documentation that that may be required for other types of work on this property. This Agreement does not authorize any work in any wetlands or other jurisdictional waters of the United States. This Agreement does not authorize any work on adjacent properties including in the City’s right-of-way. This Agreement does not authorize illicit discharges.

* Required controls (silt fence, construction entrance, etc.) are required to be installed prior to the beginning of any land disturbing activity and they must be installed properly per the Virginia Erosion and Sediment Control Handbook (VESCH). These controls must be maintained throughout the life of the project in accordance with the VESCH.
* **If there are any violations of the permit, the violations must be corrected within three calendar days of notification by the City.**
* Periodically check all controls during dry weather to insure that they are in good condition.
* Always check the controls immediately after a rainfall and clean out and repair the controls as necessary so that they will continue to function properly.
* Any sediment that travels offsite beyond the required controls must be cleaned up immediately and the area stabilized.
* All silt fence needs to remain in place until permanent vegetation is established. If silt fence has to be taken down for landscaping or seeding purposes, it must be reinstalled. If possible, plan ahead during initial silt fence installation so that silt fence placement does not interfere with stabilization operations.
* If tracking occurs onto a public street, it must be cleaned up immediately. Cleanup consist of shoveling and sweeping, not just street washing.
* If sediment washes from your site onto a public street or into a storm drain, you may be back-charged by the Public Works Department for labor and equipment costs associated with any cleanup done by the Public Works Department.
* If you have one violation or deficiency (i.e. not maintaining controls) you may then be required to provide the name of a Responsible Land Disturber associated with your project to this office.
* Excess concrete and cement should not be dumped onsite where it could potentially enter a storm drain, watercourse, or drainage ditch. This would be a violation of the Danville City Code and would be considered an illicit discharge which may result in action by the City and certain State agencies.
* All waste materials, construction debris, and trash shall be collected and either removed from the site and disposed of properly or the collected material shall be stored in a securely lidded container. If a lidded container is used, it will be emptied as necessary and its contents disposed of properly. No construction materials shall be buried onsite. A licensed sanitary waste management contractor shall collect all sanitary waste from portable units. Good housekeeping and spill control practices shall be followed during construction to eliminate storm water contamination from petroleum products, fertilizers, paints, asphalts, and concrete. A list and the location of required best management practices that are to be used to eliminate storm water contamination may be required if materials and/or fuels are stored onsite. Material storage and waste disposal shall be in compliance with federal, state, and local laws and regulations.

**Your signature states that you have reviewed this Agreement in its entirety and that you understand the requirements and that you will fully comply with all requirements of this Agreement.**

**Property Owner Signature: Date:**

**Responsible Party Signature: Date:**

**City of Danville, Virginia**

**Approved By: Date:**